Manual for EZPDA of EZ4

Please set up as the following if you want to DIY the Skin:

1. The file of “EZPDABuilder.exe” in \build\_res\ directoy:



2. All the pictures in build\_res\Res\.shell\bmp. Please make the same resolution and the same name if you want to replace those pictures as skin.

3. Please set up the position for Source Files and intent ROM

“Source Files”：\build\_res\FileSystem\.shell\bmp

intent ROM”： Generate to a file of EZPDA.gba

4. A new file of EZPDA.gba is generated after translating

5. Please rename the EZPDA.gba to ezfla\_up.bin and copy it into memory for updating the EZ4.